
=============== Test QAPIp Start ===============
PSBID :430
set_address done 
TX_mode set as bitbanging mode 2'b10 
SL_master done
initial setup done 
device_id = c22018
send command Write_enable 
erace done
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00000 : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 0 parameter write done
 write data loop-> start_address = a00001 : data = 430 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00003 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00005 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00007 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00009 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0000b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0000d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0000f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00011 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00013 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 10 parameter write done
 write data loop-> start_address = a00015 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00017 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00019 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0001b : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0001d : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0001f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00021 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00023 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00025 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00027 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 20 parameter write done
 write data loop-> start_address = a00029 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0002b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0002d : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0002f : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00031 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00033 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00035 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00037 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00039 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0003b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 30 parameter write done
 write data loop-> start_address = a0003d : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0003f : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00041 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00043 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00045 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00047 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00049 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0004b : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0004d : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0004f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 40 parameter write done
 write data loop-> start_address = a00051 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00053 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00055 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00057 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00059 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0005b : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0005d : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0005f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00061 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00063 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 50 parameter write done
 write data loop-> start_address = a00065 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00067 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00069 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0006b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0006d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0006f : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00071 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00073 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00075 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00077 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 60 parameter write done
 write data loop-> start_address = a00079 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0007b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0007d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0007f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00081 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00083 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00085 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00087 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00089 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0008b : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 70 parameter write done
 write data loop-> start_address = a0008d : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0008f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00091 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00093 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00095 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00097 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00099 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0009b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0009d : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0009f : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 80 parameter write done
 write data loop-> start_address = a000a1 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000a3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000a5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000a7 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000a9 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000ab : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000ad : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000af : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000b1 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000b3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 90 parameter write done
 write data loop-> start_address = a000b5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000b7 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000b9 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000bb : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000bd : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000bf : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000c1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000c3 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000c5 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000c7 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 100 parameter write done
 write data loop-> start_address = a000c9 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000cb : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000cd : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000cf : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d5 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d7 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d9 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000db : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 110 parameter write done
 write data loop-> start_address = a000dd : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000df : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e1 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e3 : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e4 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e8 : data = 0 : length = 0 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e8 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000ea : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000ec : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 120 parameter write done
 write data loop-> start_address = a000ee : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f0 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f2 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f4 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f6 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f8 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000fa : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000fc : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000fe : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00100 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 130 parameter write done
 write data loop-> start_address = a00102 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00104 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00106 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00108 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0010a : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0010c : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0010d : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0010f : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00110 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00111 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 140 parameter write done
 write data loop-> start_address = a00112 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00113 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00114 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00115 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00116 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00117 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00118 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00119 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011a : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011b : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 150 parameter write done
 write data loop-> start_address = a0011c : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011d : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011e : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011f : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 0 parameter write done
 write data loop-> start_address = a00120 : data = 430 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00122 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00124 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00126 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00128 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0012a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0012c : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0012e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00130 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00132 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 10 parameter write done
 write data loop-> start_address = a00134 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00136 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00138 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0013a : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0013c : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0013e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00140 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00142 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00144 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00146 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 20 parameter write done
 write data loop-> start_address = a00148 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0014a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0014c : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0014e : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00150 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00152 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00154 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00156 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00158 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0015a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 30 parameter write done
 write data loop-> start_address = a0015c : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0015e : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00160 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00162 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00164 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00166 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00168 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0016a : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0016c : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0016e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 40 parameter write done
 write data loop-> start_address = a00170 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00172 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00174 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00176 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00178 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0017a : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0017c : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0017e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00180 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00182 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 50 parameter write done
 write data loop-> start_address = a00184 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00186 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00188 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0018a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0018c : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0018e : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00190 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00192 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00194 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00196 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 60 parameter write done
 write data loop-> start_address = a00198 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0019a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0019c : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0019e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a0 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a2 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a4 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a8 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001aa : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 70 parameter write done
 write data loop-> start_address = a001ac : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ae : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b0 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b2 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b4 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b8 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ba : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001bc : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001be : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 80 parameter write done
 write data loop-> start_address = a001c0 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001c2 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001c4 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001c6 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001c8 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ca : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001cc : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ce : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001d0 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001d2 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 90 parameter write done
 write data loop-> start_address = a001d4 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001d6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001d8 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001da : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001dc : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001de : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001e0 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001e2 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001e4 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001e6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 100 parameter write done
 write data loop-> start_address = a001e8 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ea : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ec : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ee : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f0 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f2 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f4 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f6 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f8 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001fa : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 110 parameter write done
 write data loop-> start_address = a001fc : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001fe : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00200 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00202 : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00203 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00205 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00207 : data = 0 : length = 0 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00207 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00209 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0020b : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 120 parameter write done
 write data loop-> start_address = a0020d : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0020f : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00211 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00213 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00215 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00217 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00219 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0021b : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0021d : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0021f : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 130 parameter write done
 write data loop-> start_address = a00221 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00223 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00225 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00227 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00229 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0022b : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0022c : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0022e : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0022f : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00230 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 140 parameter write done
 write data loop-> start_address = a00231 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00232 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00233 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00234 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00235 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00236 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00237 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00238 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00239 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0023a : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 150 parameter write done
 write data loop-> start_address = a0023b : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0023c : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0023d : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0023e : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 0 parameter write done
 write data loop-> start_address = a0023f : data = 430 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00241 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00243 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00245 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00247 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00249 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0024b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0024d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0024f : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00251 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 10 parameter write done
 write data loop-> start_address = a00253 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00255 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00257 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00259 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0025b : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0025d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0025f : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00261 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00263 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00265 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 20 parameter write done
 write data loop-> start_address = a00267 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00269 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0026b : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0026d : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0026f : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00271 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00273 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00275 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00277 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00279 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 30 parameter write done
 write data loop-> start_address = a0027b : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0027d : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0027f : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00281 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00283 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00285 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00287 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00289 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0028b : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0028d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 40 parameter write done
 write data loop-> start_address = a0028f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00291 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00293 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00295 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00297 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00299 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0029b : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0029d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0029f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002a1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 50 parameter write done
 write data loop-> start_address = a002a3 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002a5 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002a7 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002a9 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ab : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ad : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002af : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002b1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002b3 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002b5 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 60 parameter write done
 write data loop-> start_address = a002b7 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002b9 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002bb : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002bd : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002bf : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c1 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c3 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c7 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c9 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 70 parameter write done
 write data loop-> start_address = a002cb : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002cd : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002cf : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d1 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d3 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d7 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d9 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002db : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002dd : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 80 parameter write done
 write data loop-> start_address = a002df : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e5 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e7 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e9 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002eb : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ed : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ef : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002f1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 90 parameter write done
 write data loop-> start_address = a002f3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002f5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002f7 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002f9 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002fb : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002fd : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ff : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00301 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00303 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00305 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 100 parameter write done
 write data loop-> start_address = a00307 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00309 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0030b : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0030d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0030f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00311 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00313 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00315 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00317 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00319 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 110 parameter write done
 write data loop-> start_address = a0031b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0031d : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0031f : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00321 : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00322 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00324 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00326 : data = 0 : length = 0 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00326 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00328 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0032a : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 120 parameter write done
 write data loop-> start_address = a0032c : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0032e : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00330 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00332 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00334 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00336 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00338 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0033a : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0033c : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0033e : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 130 parameter write done
 write data loop-> start_address = a00340 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00342 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00344 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00346 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00348 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034a : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034b : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034d : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034e : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034f : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 140 parameter write done
 write data loop-> start_address = a00350 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00351 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00352 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00353 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00354 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00355 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00356 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00357 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00358 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00359 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 150 parameter write done
 write data loop-> start_address = a0035a : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0035b : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0035c : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
SL_master done
TX_mode set as bitbanging mode 2'b10 

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test Power Start ===============
3V3D [V] = 3.43
3V3A [V] = 2.91
-3VA [V] = -2.97
FPGA Temprature [C] = 42.49
Elements Status(1'bQSPI,1'bSi5395Lock,1'bPPASIC_status,3'bSEU_status) = 0b110001
Power Good(1V0A,1V2A,1V8A,1V0D,1V8D) = 0b11111
channel 0: DAC [mV] = 70, ADC [mV] = 70
channel 1: DAC [mV] = 70, ADC [mV] = 70
channel 2: DAC [mV] = 70, ADC [mV] = 71
channel 3: DAC [mV] = 70, ADC [mV] = 72
channel 4: DAC [mV] = 70, ADC [mV] = 73
channel 5: DAC [mV] = 70, ADC [mV] = 67
channel 6: DAC [mV] = 70, ADC [mV] = 72
channel 7: DAC [mV] = 70, ADC [mV] = 70
channel 8: DAC [mV] = 70, ADC [mV] = 70
channel 9: DAC [mV] = 70, ADC [mV] = 70
channel a: DAC [mV] = 70, ADC [mV] = 69
channel b: DAC [mV] = 70, ADC [mV] = 70
channel c: DAC [mV] = 70, ADC [mV] = 67
channel d: DAC [mV] = 70, ADC [mV] = 68
channel e: DAC [mV] = 70, ADC [mV] = 70
channel f: DAC [mV] = 70, ADC [mV] = 72
Test Power Reseult = 1

=============== Test Clock Start ===============
10.000000000000000 0.000000 0.000000
10.017857142857142 0.000000 0.000000
10.035714285714286 0.000000 0.000000
10.053571428571429 0.000000 0.000000
10.071428571428571 0.000000 0.000000
10.089285714285714 0.000000 0.000000
10.107142857142858 0.000000 0.000000
10.125000000000000 0.000000 0.000000
10.142857142857142 0.000000 0.000000
10.160714285714286 0.000000 0.000000
10.178571428571429 0.000000 0.000000
10.196428571428571 0.000000 0.000000
10.214285714285714 0.000000 0.000000
10.232142857142858 0.000000 0.000000
10.250000000000000 0.000000 0.000000
10.267857142857142 0.000000 0.000000
10.285714285714286 0.000000 0.000000
10.303571428571429 0.000000 0.000000
10.321428571428571 0.000000 0.000000
10.339285714285714 0.000000 0.000000
10.357142857142858 0.000000 0.000000
10.375000000000000 0.000000 0.000000
10.392857142857142 0.000000 0.000000
10.410714285714286 0.000000 0.000000
10.428571428571429 0.000000 0.000000
10.446428571428571 0.000000 0.000000
10.464285714285714 0.000000 0.000000
10.482142857142858 0.000000 0.000000
10.500000000000000 0.000000 0.000000
10.517857142857142 0.000000 0.000000
10.535714285714286 0.000000 0.000000
10.553571428571429 0.000000 0.000000
10.571428571428571 0.000000 0.000000
10.589285714285714 0.000000 0.000000
10.607142857142858 0.000000 0.000000
10.625000000000000 0.000000 0.000000
10.642857142857142 0.000000 0.000000
10.660714285714286 0.000000 0.000000
10.678571428571429 0.000000 0.000000
10.696428571428571 0.000000 0.000000
10.714285714285714 0.000000 0.000000
10.732142857142858 0.000000 0.000000
10.750000000000000 0.000000 0.000000
10.767857142857142 0.000000 0.000000
10.785714285714286 0.000000 0.000000
10.803571428571429 0.000000 0.000000
10.821428571428571 0.000000 0.000000
10.839285714285714 0.000000 0.000000
10.857142857142858 0.000000 0.000000
10.875000000000000 0.000000 0.000000
10.892857142857142 0.000000 0.000000
10.910714285714286 0.000000 0.000000
10.928571428571429 0.000000 0.000000
10.946428571428571 0.000000 0.000000
10.964285714285714 0.000000 0.000000
10.982142857142858 0.000000 0.000000
11.000000000000000 0.000000 0.000000
11.017857142857142 0.000000 0.000000
11.035714285714286 0.000000 0.000000
11.053571428571429 0.000000 0.000000
11.071428571428571 0.000000 0.000000
11.089285714285714 0.000000 0.000000
11.107142857142858 0.000000 0.000000
11.125000000000000 0.000000 0.000000
11.142857142857142 0.000000 0.000000
11.160714285714286 0.000000 0.000000
11.178571428571429 0.000000 0.000000
11.196428571428571 0.000000 0.000000
11.214285714285714 0.000000 0.000000
11.232142857142858 0.000000 0.000000
11.250000000000000 0.000000 0.000000
11.267857142857142 0.000000 0.000000
11.285714285714286 0.000000 0.000000
11.303571428571429 0.000000 0.000000
11.321428571428571 0.000000 0.000000
11.339285714285714 0.000000 0.000000
11.357142857142858 0.000000 0.000000
11.375000000000000 0.000000 0.000000
11.392857142857142 0.000000 0.000000
11.410714285714286 0.000000 0.000000
11.428571428571429 0.000000 0.000000
11.446428571428571 0.000000 0.000000
11.464285714285714 0.000000 0.000000
11.482142857142858 0.000000 0.000000
11.500000000000000 0.000000 0.000000
11.517857142857142 0.000000 0.000000
11.535714285714286 0.000000 0.000000
11.553571428571429 0.000000 0.000000
11.571428571428571 0.000000 0.000000
11.589285714285714 0.000000 0.000000
11.607142857142858 0.000000 0.000000
11.625000000000000 0.000000 0.000000
11.642857142857142 0.000000 0.000000
11.660714285714286 0.000000 0.000000
11.678571428571429 0.000000 0.000000
11.696428571428571 0.000000 0.000000
11.714285714285714 0.000000 0.000000
11.732142857142858 0.000000 0.000000
11.750000000000000 0.000000 0.000000
11.767857142857142 0.000000 0.000000
11.785714285714286 1.000000 0.000000
11.803571428571429 48.000000 0.000000
11.821428571428571 467.000000 0.000000
11.839285714285714 807.000000 0.000000
11.857142857142858 995.000000 0.000000
11.875000000000000 1000.000000 0.000000
11.892857142857142 1000.000000 0.000000
11.910714285714286 1000.000000 0.000000
11.928571428571429 1000.000000 0.000000
11.946428571428571 1000.000000 0.000000
11.964285714285714 1000.000000 0.000000
11.982142857142858 1000.000000 0.000000
12.000000000000000 1000.000000 0.000000
12.017857142857142 1000.000000 0.000000
12.035714285714286 1000.000000 0.000000
12.053571428571429 1000.000000 0.000000
12.071428571428571 1000.000000 0.000000
12.089285714285714 1000.000000 0.000000
12.107142857142858 1000.000000 0.000000
12.125000000000000 1000.000000 0.000000
12.142857142857142 1000.000000 0.000000
12.160714285714286 1000.000000 0.000000
12.178571428571429 1000.000000 0.000000
12.196428571428571 1000.000000 0.000000
12.214285714285714 1000.000000 0.000000
12.232142857142858 1000.000000 0.000000
12.250000000000000 1000.000000 0.000000
12.267857142857142 1000.000000 0.000000
12.285714285714286 1000.000000 0.000000
12.303571428571429 1000.000000 0.000000
12.321428571428571 1000.000000 0.000000
12.339285714285714 1000.000000 0.000000
12.357142857142858 1000.000000 0.000000
12.375000000000000 1000.000000 0.000000
12.392857142857142 1000.000000 0.000000
12.410714285714286 1000.000000 0.000000
12.428571428571429 1000.000000 0.000000
12.446428571428571 1000.000000 0.000000
12.464285714285714 1000.000000 0.000000
12.482142857142858 1000.000000 0.000000
12.500000000000000 1000.000000 0.000000
12.517857142857142 1000.000000 0.000000
12.535714285714286 1000.000000 0.000000
12.553571428571429 1000.000000 0.000000
12.571428571428571 1000.000000 0.000000
12.589285714285714 1000.000000 0.000000
12.607142857142858 1000.000000 0.000000
12.625000000000000 1000.000000 0.000000
12.642857142857142 1000.000000 0.000000
12.660714285714286 1000.000000 0.000000
12.678571428571429 1000.000000 0.000000
12.696428571428571 1000.000000 0.000000
12.714285714285714 1000.000000 0.000000
12.732142857142858 1000.000000 0.000000
12.750000000000000 1000.000000 0.000000
12.767857142857142 1000.000000 0.000000
12.785714285714286 1000.000000 0.000000
12.803571428571429 1000.000000 0.000000
12.821428571428571 1000.000000 0.000000
12.839285714285714 1000.000000 0.000000
12.857142857142858 1000.000000 0.000000
12.875000000000000 1000.000000 0.000000
12.892857142857142 1000.000000 0.000000
12.910714285714286 1000.000000 0.000000
12.928571428571429 1000.000000 0.000000
12.946428571428571 1000.000000 0.000000
12.964285714285714 1000.000000 0.000000
12.982142857142858 1000.000000 0.000000
13.000000000000000 1000.000000 0.000000
13.017857142857142 1000.000000 0.000000
13.035714285714286 1000.000000 0.000000
13.053571428571429 1000.000000 0.000000
13.071428571428571 1000.000000 0.000000
13.089285714285714 1000.000000 0.000000
13.107142857142858 1000.000000 0.000000
13.125000000000000 1000.000000 0.000000
13.142857142857142 1000.000000 0.000000
13.160714285714286 1000.000000 0.000000
13.178571428571429 1000.000000 0.000000
13.196428571428571 1000.000000 0.000000
13.214285714285714 1000.000000 0.000000
13.232142857142858 1000.000000 0.000000
13.250000000000000 1000.000000 0.000000
13.267857142857142 1000.000000 0.000000
13.285714285714286 1000.000000 0.000000
13.303571428571429 1000.000000 0.000000
13.321428571428571 1000.000000 0.000000
13.339285714285714 1000.000000 0.000000
13.357142857142858 1000.000000 0.000000
13.375000000000000 1000.000000 0.000000
13.392857142857142 1000.000000 0.000000
13.410714285714286 1000.000000 0.000000
13.428571428571429 1000.000000 0.000000
13.446428571428571 1000.000000 0.000000
13.464285714285714 1000.000000 0.000000
13.482142857142858 1000.000000 0.000000
13.500000000000000 1000.000000 0.000000
13.517857142857142 1000.000000 0.000000
13.535714285714286 1000.000000 0.000000
13.553571428571429 1000.000000 0.000000
13.571428571428571 1000.000000 0.000000
13.589285714285714 1000.000000 0.000000
13.607142857142858 1000.000000 0.000000
13.625000000000000 1000.000000 0.000000
13.642857142857142 1000.000000 0.000000
13.660714285714286 1000.000000 0.000000
13.678571428571429 1000.000000 0.000000
13.696428571428571 1000.000000 0.000000
13.714285714285714 1000.000000 0.000000
13.732142857142858 1000.000000 0.000000
13.750000000000000 1000.000000 0.000000
13.767857142857142 1000.000000 0.000000
13.785714285714286 1000.000000 0.000000
13.803571428571429 1000.000000 0.000000
13.821428571428571 1000.000000 0.000000
13.839285714285714 1000.000000 0.000000
13.857142857142858 1000.000000 0.000000
13.875000000000000 1000.000000 0.000000
13.892857142857142 1000.000000 0.000000
13.910714285714286 1000.000000 0.000000
13.928571428571429 1000.000000 0.000000
13.946428571428571 1000.000000 0.000000
13.964285714285714 1000.000000 0.000000
13.982142857142858 1000.000000 0.000000
14.000000000000000 1000.000000 0.000000
14.017857142857142 1000.000000 0.000000
14.035714285714286 1000.000000 0.000000
14.053571428571429 1000.000000 0.000000
14.071428571428571 1000.000000 0.000000
14.089285714285714 1000.000000 0.000000
14.107142857142858 1000.000000 0.000000
14.125000000000000 1000.000000 0.000000
14.142857142857142 1000.000000 0.000000
14.160714285714286 1000.000000 0.000000
14.178571428571429 1000.000000 0.000000
14.196428571428571 1000.000000 0.000000
14.214285714285714 1000.000000 0.000000
14.232142857142858 1000.000000 0.000000
14.250000000000000 1000.000000 0.000000
14.267857142857142 1000.000000 0.000000
14.285714285714286 1000.000000 0.000000
14.303571428571429 1000.000000 0.000000
14.321428571428571 1000.000000 0.000000
14.339285714285714 1000.000000 0.000000
14.357142857142858 1000.000000 0.000000
14.375000000000000 1000.000000 0.000000
14.392857142857142 1000.000000 0.000000
14.410714285714286 1000.000000 0.000000
14.428571428571429 1000.000000 0.000000
14.446428571428571 1000.000000 0.000000
14.464285714285714 1000.000000 0.000000
14.482142857142858 1000.000000 0.000000
14.500000000000000 1000.000000 0.000000
14.517857142857142 1000.000000 0.000000
14.535714285714286 1000.000000 0.000000
14.553571428571429 1000.000000 0.000000
14.571428571428571 1000.000000 0.000000
14.589285714285714 1000.000000 0.000000
14.607142857142858 1000.000000 0.000000
14.625000000000000 1000.000000 0.000000
14.642857142857142 1000.000000 0.000000
14.660714285714286 1000.000000 0.000000
14.678571428571429 1000.000000 0.000000
14.696428571428571 1000.000000 0.000000
14.714285714285714 1000.000000 0.000000
14.732142857142858 1000.000000 0.000000
14.750000000000000 1000.000000 0.000000
14.767857142857142 1000.000000 0.000000
14.785714285714286 1000.000000 0.000000
14.803571428571429 1000.000000 0.000000
14.821428571428571 1000.000000 0.000000
14.839285714285714 1000.000000 0.000000
14.857142857142858 1000.000000 0.000000
14.875000000000000 1000.000000 0.000000
14.892857142857142 1000.000000 0.000000
14.910714285714286 1000.000000 0.000000
14.928571428571429 1000.000000 0.000000
14.946428571428571 1000.000000 0.000000
14.964285714285714 1000.000000 0.000000
14.982142857142858 1000.000000 0.000000
15.000000000000000 1000.000000 0.000000
15.017857142857142 1000.000000 0.000000
15.035714285714286 1000.000000 0.000000
15.053571428571429 1000.000000 0.000000
15.071428571428571 1000.000000 0.000000
15.089285714285714 1000.000000 0.000000
15.107142857142858 1000.000000 0.000000
15.125000000000000 1000.000000 0.000000
15.142857142857142 1000.000000 0.000000
15.160714285714286 1000.000000 0.000000
15.178571428571429 1000.000000 0.000000
15.196428571428571 1000.000000 0.000000
15.214285714285714 1000.000000 0.000000
15.232142857142858 1000.000000 0.000000
15.250000000000000 1000.000000 0.000000
15.267857142857142 1000.000000 0.000000
15.285714285714286 1000.000000 0.000000
15.303571428571429 1000.000000 0.000000
15.321428571428571 1000.000000 0.000000
15.339285714285714 1000.000000 0.000000
15.357142857142858 1000.000000 0.000000
15.375000000000000 1000.000000 0.000000
15.392857142857142 1000.000000 0.000000
15.410714285714286 1000.000000 0.000000
15.428571428571429 1000.000000 0.000000
15.446428571428571 1000.000000 0.000000
15.464285714285714 1000.000000 0.000000
15.482142857142858 1000.000000 0.000000
15.500000000000000 1000.000000 0.000000
15.517857142857142 1000.000000 0.000000
15.535714285714286 1000.000000 0.000000
15.553571428571429 1000.000000 0.000000
15.571428571428571 1000.000000 0.000000
15.589285714285714 1000.000000 0.000000
15.607142857142858 1000.000000 0.000000
15.625000000000000 1000.000000 0.000000
15.642857142857142 1000.000000 0.000000
15.660714285714286 1000.000000 0.000000
15.678571428571429 1000.000000 0.000000
15.696428571428571 1000.000000 0.000000
15.714285714285714 1000.000000 0.000000
15.732142857142858 1000.000000 0.000000
15.750000000000000 1000.000000 0.000000
15.767857142857142 1000.000000 0.000000
15.785714285714286 1000.000000 0.000000
15.803571428571429 1000.000000 0.000000
15.821428571428571 1000.000000 0.000000
15.839285714285714 1000.000000 0.000000
15.857142857142858 1000.000000 0.000000
15.875000000000000 1000.000000 0.000000
15.892857142857142 1000.000000 0.000000
15.910714285714286 1000.000000 0.000000
15.928571428571429 1000.000000 0.000000
15.946428571428571 1000.000000 0.000000
15.964285714285714 1000.000000 0.000000
15.982142857142858 1000.000000 0.000000
16.000000000000000 1000.000000 0.000000
Test Clock Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 1
always_hit_flag = 0
Autoreconfig done
----PP1----
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
----PP2----
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
----PP3----
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
----PP4----
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
----PP5----
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
----PP6----
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
----PP7----
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
----PP8----
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
0 : 1: 0
100
ASDTP : 0 times reset : result = 1
reconfig_done = 1
always_hit_flag = 0

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x0
PLLLD_fail_counter = 0x0
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6001
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001
