
=============== Test QAPIp Start ===============
PSBID :525
set_address done 
TX_mode set as bitbanging mode 2'b10 
SL_master done
initial setup done 
device_id = c22018
send command Write_enable 
erace done
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00000 : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 0 parameter write done
 write data loop-> start_address = a00001 : data = 525 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00003 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00005 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00007 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00009 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0000b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0000d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0000f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00011 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00013 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 10 parameter write done
 write data loop-> start_address = a00015 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00017 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00019 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0001b : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0001d : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0001f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00021 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00023 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00025 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00027 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 20 parameter write done
 write data loop-> start_address = a00029 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0002b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0002d : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0002f : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00031 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00033 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00035 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00037 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00039 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0003b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 30 parameter write done
 write data loop-> start_address = a0003d : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0003f : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00041 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00043 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00045 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00047 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00049 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0004b : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0004d : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0004f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 40 parameter write done
 write data loop-> start_address = a00051 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00053 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00055 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00057 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00059 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0005b : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0005d : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0005f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00061 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00063 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 50 parameter write done
 write data loop-> start_address = a00065 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00067 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00069 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0006b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0006d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0006f : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00071 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00073 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00075 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00077 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 60 parameter write done
 write data loop-> start_address = a00079 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0007b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0007d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0007f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00081 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00083 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00085 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00087 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00089 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0008b : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 70 parameter write done
 write data loop-> start_address = a0008d : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0008f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00091 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00093 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00095 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00097 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00099 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0009b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0009d : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0009f : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 80 parameter write done
 write data loop-> start_address = a000a1 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000a3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000a5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000a7 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000a9 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000ab : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000ad : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000af : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000b1 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000b3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 90 parameter write done
 write data loop-> start_address = a000b5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000b7 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000b9 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000bb : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000bd : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000bf : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000c1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000c3 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000c5 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000c7 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 100 parameter write done
 write data loop-> start_address = a000c9 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000cb : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000cd : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000cf : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d5 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d7 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000d9 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000db : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 110 parameter write done
 write data loop-> start_address = a000dd : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000df : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e1 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e3 : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e4 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e8 : data = 0 : length = 0 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000e8 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000ea : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000ec : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 120 parameter write done
 write data loop-> start_address = a000ee : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f0 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f2 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f4 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f6 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000f8 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000fa : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000fc : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a000fe : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00100 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 130 parameter write done
 write data loop-> start_address = a00102 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00104 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00106 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00108 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0010a : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0010c : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0010d : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0010f : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00110 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00111 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 140 parameter write done
 write data loop-> start_address = a00112 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00113 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00114 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00115 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00116 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00117 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00118 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00119 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011a : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011b : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 150 parameter write done
 write data loop-> start_address = a0011c : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011d : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011e : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0011f : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 0 parameter write done
 write data loop-> start_address = a00120 : data = 525 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00122 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00124 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00126 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00128 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0012a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0012c : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0012e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00130 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00132 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 10 parameter write done
 write data loop-> start_address = a00134 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00136 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00138 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0013a : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0013c : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0013e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00140 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00142 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00144 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00146 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 20 parameter write done
 write data loop-> start_address = a00148 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0014a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0014c : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0014e : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00150 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00152 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00154 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00156 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00158 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0015a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 30 parameter write done
 write data loop-> start_address = a0015c : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0015e : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00160 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00162 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00164 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00166 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00168 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0016a : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0016c : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0016e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 40 parameter write done
 write data loop-> start_address = a00170 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00172 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00174 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00176 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00178 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0017a : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0017c : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0017e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00180 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00182 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 50 parameter write done
 write data loop-> start_address = a00184 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00186 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00188 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0018a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0018c : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0018e : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00190 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00192 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00194 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00196 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 60 parameter write done
 write data loop-> start_address = a00198 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0019a : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0019c : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0019e : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a0 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a2 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a4 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001a8 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001aa : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 70 parameter write done
 write data loop-> start_address = a001ac : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ae : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b0 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b2 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b4 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001b8 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ba : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001bc : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001be : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 80 parameter write done
 write data loop-> start_address = a001c0 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001c2 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001c4 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001c6 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001c8 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ca : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001cc : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ce : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001d0 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001d2 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 90 parameter write done
 write data loop-> start_address = a001d4 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001d6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001d8 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001da : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001dc : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001de : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001e0 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001e2 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001e4 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001e6 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 100 parameter write done
 write data loop-> start_address = a001e8 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ea : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ec : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001ee : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f0 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f2 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f4 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f6 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001f8 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001fa : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 110 parameter write done
 write data loop-> start_address = a001fc : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a001fe : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00200 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00202 : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00203 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00205 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00207 : data = 0 : length = 0 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00207 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00209 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0020b : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 120 parameter write done
 write data loop-> start_address = a0020d : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0020f : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00211 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00213 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00215 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00217 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00219 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0021b : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0021d : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0021f : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 130 parameter write done
 write data loop-> start_address = a00221 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00223 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00225 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00227 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00229 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0022b : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0022c : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0022e : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0022f : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00230 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 140 parameter write done
 write data loop-> start_address = a00231 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00232 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00233 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00234 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00235 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00236 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00237 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00238 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00239 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0023a : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 150 parameter write done
 write data loop-> start_address = a0023b : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0023c : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0023d : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0023e : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 0 parameter write done
 write data loop-> start_address = a0023f : data = 525 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00241 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00243 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00245 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00247 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00249 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0024b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0024d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0024f : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00251 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 10 parameter write done
 write data loop-> start_address = a00253 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00255 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00257 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00259 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0025b : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0025d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0025f : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00261 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00263 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00265 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 20 parameter write done
 write data loop-> start_address = a00267 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00269 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0026b : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0026d : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0026f : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00271 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00273 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00275 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00277 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00279 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 30 parameter write done
 write data loop-> start_address = a0027b : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0027d : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0027f : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00281 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00283 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00285 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00287 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00289 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0028b : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0028d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 40 parameter write done
 write data loop-> start_address = a0028f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00291 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00293 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00295 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00297 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00299 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0029b : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0029d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0029f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002a1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 50 parameter write done
 write data loop-> start_address = a002a3 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002a5 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002a7 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002a9 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ab : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ad : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002af : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002b1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002b3 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002b5 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 60 parameter write done
 write data loop-> start_address = a002b7 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002b9 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002bb : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002bd : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002bf : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c1 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c3 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c7 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002c9 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 70 parameter write done
 write data loop-> start_address = a002cb : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002cd : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002cf : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d1 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d3 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d7 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002d9 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002db : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002dd : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 80 parameter write done
 write data loop-> start_address = a002df : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e5 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e7 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002e9 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002eb : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ed : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ef : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002f1 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 90 parameter write done
 write data loop-> start_address = a002f3 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002f5 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002f7 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002f9 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002fb : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002fd : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a002ff : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00301 : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00303 : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00305 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 100 parameter write done
 write data loop-> start_address = a00307 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00309 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0030b : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0030d : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0030f : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00311 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00313 : data = 2800 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00315 : data = 14 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00317 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00319 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 110 parameter write done
 write data loop-> start_address = a0031b : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0031d : data = b300 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0031f : data = 93b8 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00321 : data = 1 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00322 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00324 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00326 : data = 0 : length = 0 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00326 : data = 0 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00328 : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0032a : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 120 parameter write done
 write data loop-> start_address = a0032c : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0032e : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00330 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00332 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00334 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00336 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00338 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0033a : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0033c : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0033e : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 130 parameter write done
 write data loop-> start_address = a00340 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00342 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00344 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00346 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00348 : data = e6 : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034a : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034b : data = ffff : length = 2 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034d : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034e : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0034f : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 140 parameter write done
 write data loop-> start_address = a00350 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00351 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00352 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00353 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00354 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00355 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00356 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00357 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00358 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a00359 : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
No. 150 parameter write done
 write data loop-> start_address = a0035a : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0035b : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
write data loop-> start_address = a0035c : data = 0 : length = 1 
send command Write_enable 
0 th read status = 0 
wip check ok 
SL_master done
TX_mode set as bitbanging mode 2'b10 

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 0

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5000
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x70
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 0

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 0

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x70
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5000
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x70
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5000
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 0

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 1024
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 2048

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 0
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 3072
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 1024

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x70
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1

=============== Test ASDTP Start ===============
reconfig_done = 0
always_hit_flag = 2048
Autoreconfig fail
ASDTP : 10 times reset : result = 2
reconfig_done = 0
always_hit_flag = 3072

------- Done check -------
Si_done = 0x1
LOLB_in = 0x1
PPconfig_done = 0xff
PPconfig_error = 0x60
PLLLD_fail_counter = 0xa
PPconfig_fail_counter = 0x0
PP1_PLLLD = 0x1001
PP2_PLLLD = 0x2001
PP3_PLLLD = 0x3001
PP4_PLLLD = 0x4001
PP5_PLLLD = 0x5001
PP6_PLLLD = 0x6000
PP7_PLLLD = 0x7001
PP8_PLLLD = 0x8001

=============== Test Recov Start ===============
Test Recov Result = 1
